ULTRAPEN™ PT™ and PTBT™ Series Pocket Testers

Get benchtop lab accuracy in easy-to-use, easy-to-maintain, wireless handheld instruments. Select from a variety of water quality pocket testers, each featuring simultaneous measurement of Temperature and one critical parameter:

* PT1 and PTBT1 measure COND, TDS, and Salinity.
* PT2 and PTBT2 measure pH.
* PT3 and PTBT3 measure ORP.
* PT4 and PTBT4 measure Free Chlorine Equivalent (FCE™).
* PT5 and PTBT5 measure Dissolved Oxygen.
* PT6 and PTBT6 measure Nitrate.

Original PT Series instruments feature one-button measurements and calibration while the new PTBT Series pairs with your Android™ or iPhone® Bluetooth®-enabled device allowing you to control your instrument from the PTBTX2™ mobile application.